LOOKING FOR WORK OVER RIG XJ450HP SPARE PARTS

RFQ DEADLINE: Feb.5th.2016.

|  |  |
| --- | --- |
| **Model**  | XJ 450 |
| **Rating hook load** | 800 KN |
| **Mast Height** | 35 m |
| **String Up** | 5X4 |
| **Height of substructure floor** | 4.5 m |
| **Mass** | 52 Ton |
| **Vin** | LA9YEPCE9E0DFX003 |
| **Serial No.** | 15293 |
| **Max Hook load** | 1125 KN |
| **Input horse Power** | 400-550 KW |
| **Wire line Diameter** | 26 mm |
| **Hook Speed** | 0.23-1.5 m/sec |
| **Max Road Speed**  | 45 km/h |
| **Rotary table open hole size** | 444.5 mm |

# REQUIRED ON RIG SITE:

1：DERRICK LOCK SPRING FOR WORK OVER RIG XJ 450HP, Length: 85 cm, ID: 43.43mm, wire diameter(OD): 8.03mm---- QTY 10

2：   SPRING FOR MAST SYSTEM FOR WORK OVER RIG XJ 450 HP, Length: 30 cm, Diameter(ID): 23.3mm cm, Diameter of wire(OD): 4.02mm—QTY 10

NOTE: As per our RFQ , FYR , Pls consider the followings:

* For item No .1 (1045308).this spring install on mast system exactly on Derrick and it call derrick lock spring
* For item No. 2 (104500549).  this spring install on mast system between two section (upper and lower section).